TOP SECRET COATINGS                       MATERIAL SAFETY DATA SHEET
1999 ELIZABETH ST.			            FOR COATINGS AND RELATED MATERIALS
NO.BRUNSWICK, NJ 08902                    PREP: FEB. 1999    UPDATE: CURRENT

+----------------------------------------+  +----------------------------------+
| SECTION I  PRODUCT IDENTIFICATION      |  |   24 HOUR EMERGENCY ASSISTANCE   |
|----------------------------------------|  |----------------------------------|
|                                        |  |EMERGENCY  (360)-631-3171         |
| PRODUCT NUMBER:  TS-6990               |  |INFO:    (TOP SECRET)(360)651-9050|
|                                        |  |----------------------------------|
| PRODUCT NAME: URETHANE AQUEOUS	 	|  |  HAZARD RATING |  THIS PRODUCT   |
|                FINISH	 			|  |   0   LOWEST   | HEALTH        2 |
|                			 		|  |   1     |      | FLAMMABILITY  1 |
|                                        |  |   2     |      | REACTIVITY    0 |
| PRODUCT CLASS: SELF CROSSLINKING       |  |   3     |      | PERSONAL        |
|                AROMATIC URETHANE       |  |   4   EXTREME  |  PROTECTION   B |
+----------------------------------------+  +----------------------------------+
+------------------------------------------------------------------------------+
| SECTION II  HAZARDOUS INGREDIENTS                                            |
|------------------------------------------------------------------------------|
| INGREDIENT                  CAS NUMBER    PERCENT     OCCUPATIONAL EXPOSURE  |
|                                         (BY WEIGHT)   TLV(ACGIH)  PEL(OSHA)  |
+------------------------------------------------------------------------------+

  1-METHYL-2-PYRROLIDINONE;
    N-METHYL PYRROLIDONE       872-50-4      5-10%        100ppm     100ppm

  N-N-DIMETHYLETHANOLAMINE     108-01-0      1-5%           5ppm      10ppm

  * DI-PROPYLENE GLYCOL
       METHYL ETHER              N/A         1-5%         100ppm     100ppm

   "PURSUANT TO TITLE III OF THE SUPERFUND AMENDMENTS AND REAUTHORIZATION ACT OF 1986 (SARA) AND
    40 CFR PART 372, THIS PRODUCT CONTAINS OR MAY CONTAIN A TOXIC CHEMICAL IN A QUANTITY SUBJECT
    TO THE REPORTING REQUIREMENTS UNDER SECTION 313"
+------------------------------------------------------------------------------+
| SECTION III  PHYSICAL DATA                                                   |
+------------------------------------------------------------------------------+
BOILING RANGE: 192-396 F.                     VAPOR PRESSURE: 83mmHg@20C
VAPOR DENSITY:      HEAVIER THAN AIR: XX      LIGHTER THAN AIR:     
EVAPORATION RATE:  FASTER THAN ETHER:        SLOWER THAN ETHER: XX  
                                             SOLUBILITY IN WATER: YES
VOC: 71 GRAMS/LITER (LESS WATER)             REACTIVITY IN WATER: NO
WEIGHT/GALLON: 8.82 lbs.
APPEARANCE & ODOR:  Thin milky white liquid with a slight mild sweet odor.
+------------------------------------------------------------------------------+
| SECTION IV  FIRE AND EXPLOSION HAZARD DATA                                   |
+------------------------------------------------------------------------------+
DOT PROPER SHIPPING NAME:  PAINT          FLASH POINT: >200 F.     % LEL: 1.2
FLAMMABILITY CLASSIFICATION:   OSHA: NONFLAMMABLE LIQUID
HAZARD CLASS: NOT REGULATED     DOT: NONFLAMMABLE LIQUID

EXTINGUISHING MEDIA: Foam, Carbon Dioxide, Dry Chemical, Water Fog.

UNUSUAL FIRE AND EXPLOSION HAZARDS: Material in itself is normally stable but
can become unstable at elevated temperatures and pressures, or may react with
water with some release of energy but not violently.

SPECIAL FIREFIGHTING PROCEDURES: Water may be used to cool and protect exposed
containers to prevent pressure build up.

SECTION V:  HEALTH HAZARD DATA                                                                                                   
PRIMARY ROUTE(S) OF EXPOSURE:  INHALATION, SKIN OR EYE CONTACT, INGESTION.

EFFECTS OF ACUTE OVEREXPOSURE:

INHALATION:  PROLONGED INHALATION, IN CONFINED AREAS, MAY LEAD TO MUCOUS MEMBRANE IRRITATION, DIZZINESS, HEADACHE.
SKIN CONTACT:  IRRITATION OF THE SKIN.
EYE CONTACT:  IRRITATION OF THE EYES.
INGESTION:  AMOUNTS INGESTED INCIDENTAL TO CONSUMER AND INDUSTRIAL HANDLING ARE NOT LIKELY TO CAUSE INJURY. HOWEVER, INGESTION OF LARGER AMOUNTS COULD CAUSE SERIOUS INJURY.

EMERGENCY AND FIRST AID PROCEDURES:

INHALATION:  REMOVE TO FRESH AIR.IF RESPIRATORY SYMPTOMS DEVELOP, SEEK MEDICAL ATTENTION AT ONCE.
SKIN CONTACT:  WASH OFF QUICKLY WITH PLENTY OF WATER, THEN SOAP AND WATER.  REMOVE AND WASH CONTAMINATED CLOTHING BEFORE REUSE.
EYE CONTACT:  FLUSH IMMEDIATELY WITH LARGE AMOUNTS OF WATER, ESPECIALLY UNDER LIDS, FOR AT LEAST 15 MINUTES. OBTAIN EMERGENCY MEDICAL TREATMENT.
INGESTION:  IF SWALLOWED, OBTAIN MEDICAL TREATMENT IMMEDIATELY.

MEDICAL CONDITIONS AGGRAVATED BY CHRONIC OVEREXPOSURE: NONE, WHEN USED IN ACCORDANCE WITH SAFE HANDLING INSTRUCTIONS.(SEE SECTION VIII)

CARCINOGENICITY:  THIS PRODUCT CONTAINS NO KNOWN CARCINOGENS IN REPORTABLE QUANTITIES AS DEFINED BY NTP, IARC, OSHA, EPA.

SECTION VI:  REACTIVITY DATA

STABILITY:   UNSTABLE:    STABLE: XX  HAZARDOUS POLYMERIZATION: MAY OCCUR:    WILL NOT OCCUR: XX 

HAZARDOUS DECOMPOSITION PRODUCTS:  CARBON MONOXIDE AND CARBON DIOXIDE.

CONDITIONS TO AVOID:  ELEVATED TEMPERATURES, CONTACT WITH OXIDIZING AGENTS.

INCOMPATIBILITY:  OXIDIZERS AND/OR HYDROFLUORIC ACID.

SECTION VII: SPILL OR LEAK PROCEDURES

STEPS TO BE TAKEN IN CASE MATERIAL IS RELEASED OR SPILLED:  COMPLY WITH ALL APPLICABLE HEALTH AND ENVIRONMENTAL REGULATIONS. VENTILATE AREA. SPILLS MAY BE COLLECTED WITH ABSORBENT MATERIALS.

WASTE DISPOSAL: DISPOSE OF ACCORDING TO LOCAL, STATE AND FEDERAL REGULATIONS. AVOID DISCHARGE TO NATURAL WATERS.

SECTION VIII: SAFE HANDLING AND USE INFORMATION                                                      
USE ONLY WITH ADEQUATE VENTILATION. AVOID BREATHING VAPOR AND SPRAY MIST. AVOID CONTACT WITH SKIN AND EYES.

VENTILATION:  LOCAL EXHAUST PREFERABLE. GENERAL EXHAUST ACCEPTABLE IF THE EXPOSURE TO MATERIALS IN SECTION II IS MAINTAINED BELOW APPLICABLE EXPOSURE LIMITS.

RESPIRATORY PROTECTION:  IF PERSONAL EXPOSURE CANNOT BE CONTROLLED BELOW APPLICABLE LIMITS BY VENTILATION, WEAR A PROPERLY FITTED ORGANIC VAPOR/PARTICULATE RESPIRATOR APPROVED BY NIOSH/OSHA FOR PROTECTION AGAINST MATERIALS IN SECTION II.

PROTECTIVE GLOVES:  WEAR GLOVES WHICH ARE RECOMMENDED BY GLOVE SUPPLIER FOR PROTECTION AGAINST MATERIALS IN SECTION II.

EYE PROTECTION:  WEAR SAFETY SPECTACLES WITH UNPERFORATED SIDESHIELDS.

PERSONAL PROTECTIVE EQUIPMENT:  EYE WASH - SAFETY SHOWERS - GOGGLES - SAFETY GLASSES - IMPERVIOUS GLOVES.

HYGIENIC PRACTICES:  KEEP WORK AREA CLEAN AND FREE FROM SPILLS AND LEAKS.  ALWAYS WASH HANDS THOROUGHLY WITH SOAP AND WATER BEFORE HANDLING FOOD, DRINK OR SMOKING.

SECTION IX:  SPECIAL PRECAUTIONS  
KEEP OUT OF THE REACH OF CHILDREN

PRECAUTIONS TO BE TAKEN IN HANDLING AND STORING:  AVOID TEMPERATURES BELOW 40 F. KEEP FROM FREEZING. STORE CONTAINERS WITH LIDS TIGHTLY CLOSED AND APPROPRIATELY LABELED.

SECTION X:  SUPPLEMENTAL INFORMATION

NOTE:  THIS PRODUCT CONTAINS NO MERCURY IN REPORTABLE QUANTITIES AS DEFINED BY OSHA AND EPA.

THE INFORMATION IN THIS DATA SHEET IS BELIEVED TO BE ACCURATE AND TRUE AT THE TIME OF PREPARATION OF THIS DOCUMENT.  THIS IS NOT A WARRANTY OF PRODUCT OR PRODUCT SPECIFICATION.  THE END-USER OF THIS PRODUCT IS ADVISED TO VERIFY IN ADVANCE THAT THE INFORMATION IN THIS SHEET IS CURRENT, APPLICABLE, AND SUITABLE TO THEIR CIRCUMSTANCES.